Open the .hwx file for firmware you want to use.

This will usually be in (Subsistute AS46 for you AS version)

C:\BrAutomation\**AS46**\AS\Hardware\Modules\X20DS438A\

Open the file X20DS438A.hwx

Replace the following 4 lines of code.

Search for

**<Channel ID="InputData01\_6" HwdResource="IO" FromVersion="D3.09"**

Replace the ext property

<Parameter ID="Ext" Value="/GROUP=0x1105:8;0x1107:8;0x1109:8;0x110b:8;0x110d:8;0x110f:8" Type="STRING"/>

**<Channel ID="InputData02\_6" HwdResource="IO" FromVersion="D3.09"**

<Parameter ID="Ext" Value="/GROUP=0x1505:8;0x1507:8;0x1509:8;0x150b:8;0x150d:8;0x150f:8" Type="STRING"/>

**<Channel ID="InputData03\_6" HwdResource="IO" FromVersion="D3.09"**

<Parameter ID="Ext" Value="/GROUP=0x1905:8;0x1907:8;0x1909:8;0x190b:8;0x190d:8;0x190f:8" Type="STRING"/>

**<Channel ID="InputData04\_6" HwdResource="IO" FromVersion="D3.09"**

<Parameter ID="Ext" Value="/GROUP=0x1d05:8;0x1d07:8;0x1d09:8;0x1d0b:8;0x1d0d:8;0x1d0f:8" Type="STRING"/>